Frigidaire FFRA0511R1 5, 000 BTU 115V Window-Mounted Mini-Compact Air Conditioner with Mechanical Controls



* 5,000 BTU mini-compact air conditioner for window-mounted installation uses standard 115V electrical outlet (Window mounting kit included)
* Quickly cools a room up to 150 sq. ft. with dehumidification up to 1.1 pints per hour
* Mechanical rotary controls, 2 cool speeds, 2 fan speeds, and 2-way air direction
* Low power start-up, quiet operation and effortless restart
* Energy Efficiency Ratio (EER): 11.1. Please note: This product is an Air Conditioner and not a Swamp Cooler. Swamp coolers will only perform only in high humidity regions such as the Southwest part of the US.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
|  |  |  |  |  |  |
| Model | FFRA0511R1 | FFRA0811R1 | FFRH0822R1 | FFRA1022R1 | FFRA1222R1 | FFRH1222R2 |
| BTUs | 5,000 | 8,000 | 8,000 | 10,000 | 12,000 | 12,000 |
| Room Size | 150 sq. ft. | 350 sq. ft. | 350 sq. ft. | 450 sq. ft. | 550 sq. ft. | 550 sq. ft. |
| Cooling Speeds | 2 | 3 | 3 | 3 | 3 | 3 |
| Fan Speeds | 2 | 3 | 3 | 3 | 3 | 3 |
| Energy Saver Mode |  |  | ✓ | ✓ | ✓ | ✓ |
| Sleep Mode |  |  | ✓ | ✓ | ✓ | ✓ |
| Timer |  |  | ✓ | ✓ | ✓ | ✓ |
| Auto-Restart |  | ✓ | ✓ |  | ✓ | ✓ |
| Air Direction Control | 2 | 8 | 8 | 8 | 8 | 8 |