|  |
| --- |
| https://images-na.ssl-images-amazon.com/images/S/aplus-seller-content-images-us-east-1/ATVPDKIKX0DER/A5D5QHQMB730E/B00QXSC3V2/fOPTsLRBRAun._UX970_TTW_.jpg |

The Koldfront 18,500 BTU Heat/Cool Window Air Conditioner(**WAC18001W**) can service a space up to 1,000 square feet with cool air during the warm summer months and heat during the winter. The air conditioner has 18,500 BTUs of cooling power and 16,000 BTUs of electric heating power. Using the electronic thermostat and digital display, you can set your desired temperature as well as control other convenient features like the energy saver mode, fan speed and 24 hour timer.  
  
**Energy Saver Mode:**  
This function cycles the fan on for two minutes at 10 minute intervals and will turn the compressor back on if the the room temperature exceeds the set temperature  
  
**Digital Display with Dehumidifier:**  
A control panel with digital temperature display and three (3) fan speeds lets you control airflow, with a dehumidifying mode to dry your space  
  
**Sleep Function:**  
To save energy, sleep mode will adjust the temperature periodically before returning to the set temperature after six (6) hours  
  
**Remote Control:**  
Operate the temperature setting and fan speed from anywhere in the room with the convenient remote control

|  |
| --- |
| https://images-na.ssl-images-amazon.com/images/S/aplus-seller-content-images-us-east-1/ATVPDKIKX0DER/A5D5QHQMB730E/B00QXR9794/QjhziwGOR7m6._UX847_TTW_.jpg |

**Specifications**

* Model: WAC18001W
* 18,500 BTU cooling – 7.7A/1730W
* 16,000 BTU heating – 20.0A/4800W
* Coverage area: 1,000 sq. ft. (cool) 700 sq. ft. (heat)
* Four (4) operating modes including Dry Mode for dehumidifying
* Three (3) fan speeds with auto option
* 24-hour timer
* Digital thermostat-controlled heating and cooling
* Maintains temperatures between 62° F (17° C) and 86° F (30° C)
* Installation hardware and weather seals included
* Four-way air directional louvers
* Input voltage: 220 V/60 Hz
* Weight: 117 lbs
* Fits windows between 31 & 42” wide
* Minimum window height: 19.5”
* Dimensions: 17.9" H x 23.6" W x 25.4" D